#MicroXplorer Configuration settings - do not modify
ADC1.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_1
ADC1.CommonPathInternal=null|null|null|null
ADC1.IPParameters=Rank-0\#ChannelRegularConversion,Channel-0\#ChannelRegularConversion,SamplingTime-0\#ChannelRegularConversion,OffsetNumber-0\#ChannelRegularConversion,NbrOfConversionFlag,master,CommonPathInternal
ADC1.NbrOfConversionFlag=1
ADC1.OffsetNumber-0\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.Rank-0\#ChannelRegularConversion=1
ADC1.SamplingTime-0\#ChannelRegularConversion=ADC_SAMPLETIME_2CYCLES_5
ADC1.master=1
ADC2.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_2
ADC2.CommonPathInternal=null|null|null|null
ADC2.IPParameters=Rank-0\#ChannelRegularConversion,Channel-0\#ChannelRegularConversion,SamplingTime-0\#ChannelRegularConversion,OffsetNumber-0\#ChannelRegularConversion,NbrOfConversionFlag,CommonPathInternal
ADC2.NbrOfConversionFlag=1
ADC2.OffsetNumber-0\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC2.Rank-0\#ChannelRegularConversion=1
ADC2.SamplingTime-0\#ChannelRegularConversion=ADC_SAMPLETIME_2CYCLES_5
CAD.formats=
CAD.pinconfig=
CAD.provider=
FDCAN1.CalculateBaudRateNominal=800000
FDCAN1.CalculateTimeBitNominal=1250
FDCAN1.CalculateTimeQuantumNominal=250.0
FDCAN1.IPParameters=CalculateTimeQuantumNominal,CalculateTimeBitNominal,CalculateBaudRateNominal
FMC.BusTurnAroundDuration1=2
FMC.BusTurnAroundDuration2=2
FMC.BusTurnAroundDuration3=2
FMC.DataSetupTime1=30
FMC.DataSetupTime2=30
FMC.DataSetupTime3=30
FMC.IPParameters=WriteOperation3,WriteOperation1,WriteOperation2,MaxChipSelectPulse3,DataSetupTime3,BusTurnAroundDuration3,DataSetupTime2,BusTurnAroundDuration2,DataSetupTime1,BusTurnAroundDuration1
FMC.MaxChipSelectPulse3=DISABLE
FMC.WriteOperation1=FMC_WRITE_OPERATION_ENABLE
FMC.WriteOperation2=FMC_WRITE_OPERATION_ENABLE
FMC.WriteOperation3=FMC_WRITE_OPERATION_ENABLE
FREERTOS.FootprintOK=true
FREERTOS.IPParameters=Tasks01,FootprintOK
FREERTOS.Tasks01=taskEPS,24,256,taskEPSRunner,Default,NULL,Static,taskEPSBuffer,taskEPSControlBlock;taskSnap,48,512,taskSnapRunner,Default,NULL,Static,taskSnapBuffer,taskSnapControlBlock;taskAI,24,37968,taskAIRunner,Default,NULL,Static,taskAIBuffer,taskAIControlBlock
File.Version=6
GPIO.groupedBy=Group By Peripherals
I2C1.IPParameters=Timing
I2C1.Timing=0x00707CBB
I2C3.IPParameters=Timing
I2C3.Timing=0x00707CBB
KeepUserPlacement=false
Mcu.CPN=STM32L552ZET3
Mcu.ContextProject=TrustZoneDisabled
Mcu.Family=STM32L5
Mcu.IP0=ADC1
Mcu.IP1=ADC2
Mcu.IP10=NVIC
Mcu.IP11=PWR
Mcu.IP12=RCC
Mcu.IP13=SPI1
Mcu.IP14=SPI2
Mcu.IP15=SYS
Mcu.IP16=TIM7
Mcu.IP17=UART4
Mcu.IP18=USART1
Mcu.IP19=USART2
Mcu.IP2=DEBUG
Mcu.IP20=USART3
Mcu.IP21=USB
Mcu.IP22=USB_DEVICE
Mcu.IP3=FDCAN1
Mcu.IP4=FMC
Mcu.IP5=FREERTOS
Mcu.IP6=GTZC
Mcu.IP7=I2C1
Mcu.IP8=I2C3
Mcu.IP9=ICACHE
Mcu.IPNb=23
Mcu.Name=STM32L552ZETx
Mcu.Package=LQFP144
Mcu.Pin0=PE2
Mcu.Pin1=PE3
Mcu.Pin10=PF2
Mcu.Pin100=PB8
Mcu.Pin101=PB9
Mcu.Pin102=PE0
Mcu.Pin103=PE1
Mcu.Pin104=VP_FREERTOS_VS_CMSIS_V2
Mcu.Pin105=VP_GTZC_VS_GTZC_Enable
Mcu.Pin106=VP_ICACHE_VS_ICACHE
Mcu.Pin107=VP_PWR_VS_DBSignals
Mcu.Pin108=VP_PWR_VS_SECSignals
Mcu.Pin109=VP_SYS_VS_tim2
Mcu.Pin11=PF3
Mcu.Pin110=VP_TIM7_VS_ClockSourceINT
Mcu.Pin111=VP_USB_DEVICE_VS_USB_DEVICE_CDC_FS
Mcu.Pin12=PF4
Mcu.Pin13=PF5
Mcu.Pin14=PF6
Mcu.Pin15=PF7
Mcu.Pin16=PF8
Mcu.Pin17=PF9
Mcu.Pin18=PF10
Mcu.Pin19=PH0-OSC_IN (PH0)
Mcu.Pin2=PE4
Mcu.Pin20=PH1-OSC_OUT (PH1)
Mcu.Pin21=PC0
Mcu.Pin22=PC1
Mcu.Pin23=PC2
Mcu.Pin24=PC3
Mcu.Pin25=PA0
Mcu.Pin26=PA1
Mcu.Pin27=PA2
Mcu.Pin28=PA3
Mcu.Pin29=PA4
Mcu.Pin3=PE5
Mcu.Pin30=PA5
Mcu.Pin31=PA6
Mcu.Pin32=PA7
Mcu.Pin33=PC4
Mcu.Pin34=PC5
Mcu.Pin35=PB0
Mcu.Pin36=PB1
Mcu.Pin37=PB2
Mcu.Pin38=PF11
Mcu.Pin39=PF12
Mcu.Pin4=PE6
Mcu.Pin40=PF13
Mcu.Pin41=PF14
Mcu.Pin42=PF15
Mcu.Pin43=PG0
Mcu.Pin44=PG1
Mcu.Pin45=PE7
Mcu.Pin46=PE8
Mcu.Pin47=PE9
Mcu.Pin48=PE10
Mcu.Pin49=PE11
Mcu.Pin5=PC13
Mcu.Pin50=PE12
Mcu.Pin51=PE13
Mcu.Pin52=PE14
Mcu.Pin53=PE15
Mcu.Pin54=PB10
Mcu.Pin55=PB12
Mcu.Pin56=PB13
Mcu.Pin57=PB14
Mcu.Pin58=PB15
Mcu.Pin59=PD8
Mcu.Pin6=PC14-OSC32_IN (PC14)
Mcu.Pin60=PD9
Mcu.Pin61=PD10
Mcu.Pin62=PD11
Mcu.Pin63=PD12
Mcu.Pin64=PD13
Mcu.Pin65=PD14
Mcu.Pin66=PD15
Mcu.Pin67=PG2
Mcu.Pin68=PG3
Mcu.Pin69=PG4
Mcu.Pin7=PC15-OSC32_OUT (PC15)
Mcu.Pin70=PG5
Mcu.Pin71=PG6
Mcu.Pin72=PG7
Mcu.Pin73=PG8
Mcu.Pin74=PC6
Mcu.Pin75=PC7
Mcu.Pin76=PA8
Mcu.Pin77=PA9
Mcu.Pin78=PA10
Mcu.Pin79=PA11
Mcu.Pin8=PF0
Mcu.Pin80=PA12
Mcu.Pin81=PA13 (JTMS/SWDIO)
Mcu.Pin82=PA14 (JTCK/SWCLK)
Mcu.Pin83=PD0
Mcu.Pin84=PD1
Mcu.Pin85=PD2
Mcu.Pin86=PD3
Mcu.Pin87=PD4
Mcu.Pin88=PD5
Mcu.Pin89=PD7
Mcu.Pin9=PF1
Mcu.Pin90=PG9
Mcu.Pin91=PG10
Mcu.Pin92=PG11
Mcu.Pin93=PG12
Mcu.Pin94=PG13
Mcu.Pin95=PG14
Mcu.Pin96=PG15
Mcu.Pin97=PB5
Mcu.Pin98=PB6
Mcu.Pin99=PB7
Mcu.PinsNb=112
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32L552ZETx
MxCube.Version=6.9.0
MxDb.Version=DB.6.0.90
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.PendSV_IRQn=true\:7\:0\:false\:false\:false\:true\:false\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_3
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false\:false
NVIC.SavedPendsvIrqHandlerGenerated=true
NVIC.SavedSvcallIrqHandlerGenerated=true
NVIC.SavedSystickIrqHandlerGenerated=true
NVIC.SysTick_IRQn=true\:7\:0\:false\:false\:false\:true\:false\:true\:false
NVIC.TIM2_IRQn=true\:7\:0\:false\:false\:true\:false\:false\:true\:true
NVIC.TimeBase=TIM2_IRQn
NVIC.TimeBaseIP=TIM2
NVIC.USB_FS_IRQn=true\:5\:0\:false\:false\:true\:true\:false\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
PA0.GPIOParameters=GPIO_Speed
PA0.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA0.Mode=Asynchronous
PA0.Signal=UART4_TX
PA1.GPIOParameters=GPIO_Speed
PA1.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA1.Mode=Asynchronous
PA1.Signal=UART4_RX
PA10.GPIOParameters=GPIO_Speed
PA10.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA10.Mode=Asynchronous
PA10.Signal=USART1_RX
PA11.Mode=Device
PA11.Signal=USB_DM
PA12.Mode=Device
PA12.Signal=USB_DP
PA13\ (JTMS/SWDIO).Mode=Serial_Wire
PA13\ (JTMS/SWDIO).Signal=DEBUG_JTMS-SWDIO
PA14\ (JTCK/SWCLK).Mode=Serial_Wire
PA14\ (JTCK/SWCLK).Signal=DEBUG_JTCK-SWCLK
PA2.GPIOParameters=GPIO_Speed
PA2.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA2.Mode=Asynchronous
PA2.Signal=USART2_TX
PA3.GPIOParameters=GPIO_Speed
PA3.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA3.Mode=Asynchronous
PA3.Signal=USART2_RX
PA4.Locked=true
PA4.Mode=NSS_Signal_Hard_Output
PA4.Signal=SPI1_NSS
PA5.Locked=true
PA5.Mode=Full_Duplex_Master
PA5.Signal=SPI1_SCK
PA6.Locked=true
PA6.Mode=Full_Duplex_Master
PA6.Signal=SPI1_MISO
PA7.Locked=true
PA7.Signal=ADCx_IN12
PA8.Locked=true
PA8.Signal=GPIO_Output
PA9.GPIOParameters=GPIO_Speed
PA9.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB0.Locked=true
PB0.Signal=ADCx_IN15
PB1.Locked=true
PB1.Signal=ADCx_IN16
PB10.GPIOParameters=GPIO_Speed
PB10.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PB10.Locked=true
PB10.Mode=Asynchronous
PB10.Signal=USART3_TX
PB12.Locked=true
PB12.Mode=NSS_Signal_Hard_Output
PB12.Signal=SPI2_NSS
PB13.Locked=true
PB13.Mode=Full_Duplex_Master
PB13.Signal=SPI2_SCK
PB14.Locked=true
PB14.Mode=Full_Duplex_Master
PB14.Signal=SPI2_MISO
PB15.Locked=true
PB15.Mode=Full_Duplex_Master
PB15.Signal=SPI2_MOSI
PB2.Locked=true
PB2.Signal=GPIO_Output
PB5.Locked=true
PB5.Mode=Full_Duplex_Master
PB5.Signal=SPI1_MOSI
PB6.Locked=true
PB6.Mode=I2C
PB6.Signal=I2C1_SCL
PB7.Locked=true
PB7.Mode=I2C
PB7.Signal=I2C1_SDA
PB8.Locked=true
PB8.Mode=FDCAN_Activate
PB8.Signal=FDCAN1_RX
PB9.Locked=true
PB9.Mode=FDCAN_Activate
PB9.Signal=FDCAN1_TX
PC0.Locked=true
PC0.Signal=ADCx_IN1
PC1.Locked=true
PC1.Signal=ADCx_IN2
PC13.Locked=true
PC13.Signal=GPIO_Output
PC14-OSC32_IN\ (PC14).Mode=LSE-External-Oscillator
PC14-OSC32_IN\ (PC14).Signal=RCC_OSC32_IN
PC15-OSC32_OUT\ (PC15).Mode=LSE-External-Oscillator
PC15-OSC32_OUT\ (PC15).Signal=RCC_OSC32_OUT
PC2.Locked=true
PC2.Signal=ADCx_IN3
PC3.Locked=true
PC3.Signal=ADCx_IN4
PC4.Locked=true
PC4.Signal=ADCx_IN13
PC5.GPIOParameters=GPIO_Speed
PC5.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PC5.Locked=true
PC5.Mode=Asynchronous
PC5.Signal=USART3_RX
PC6.Locked=true
PC6.Signal=GPIO_Output
PC7.GPIOParameters=GPIO_Speed,GPIO_PuPd
PC7.GPIO_PuPd=GPIO_NOPULL
PC7.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PC7.Locked=true
PC7.Signal=GPIO_Output
PD0.Signal=FMC_D2_DA2
PD1.Signal=FMC_D3_DA3
PD10.Signal=FMC_D15_DA15
PD11.Signal=FMC_A16_CLE
PD12.Signal=FMC_A17_ALE
PD13.Signal=FMC_A18
PD14.Signal=FMC_D0_DA0
PD15.Signal=FMC_D1_DA1
PD2.Locked=true
PD2.Signal=SDMMC1_CMD
PD3.Locked=true
PD3.Signal=GPIO_Output
PD4.Signal=FMC_NOE
PD5.Signal=FMC_NWE
PD7.Mode=NorPsramChipSelect1_1
PD7.Signal=FMC_NE1
PD8.Signal=FMC_D13_DA13
PD9.Signal=FMC_D14_DA14
PE0.Signal=FMC_NBL0
PE1.Signal=FMC_NBL1
PE10.Signal=FMC_D7_DA7
PE11.Signal=FMC_D8_DA8
PE12.Signal=FMC_D9_DA9
PE13.Signal=FMC_D10_DA10
PE14.Signal=FMC_D11_DA11
PE15.Signal=FMC_D12_DA12
PE2.Signal=FMC_A23
PE3.Signal=FMC_A19
PE4.Signal=FMC_A20
PE5.Signal=FMC_A21
PE6.Signal=FMC_A22
PE7.Signal=FMC_D4_DA4
PE8.Signal=FMC_D5_DA5
PE9.Signal=FMC_D6_DA6
PF0.Signal=FMC_A0
PF1.Signal=FMC_A1
PF10.GPIOParameters=GPIO_PuPd
PF10.GPIO_PuPd=GPIO_NOPULL
PF10.Locked=true
PF10.Signal=GPIO_Input
PF11.GPIOParameters=GPIO_PuPd
PF11.GPIO_PuPd=GPIO_NOPULL
PF11.Locked=true
PF11.Signal=GPIO_Output
PF12.Signal=FMC_A6
PF13.Signal=FMC_A7
PF14.Signal=FMC_A8
PF15.Signal=FMC_A9
PF2.Signal=FMC_A2
PF3.Signal=FMC_A3
PF4.Signal=FMC_A4
PF5.Signal=FMC_A5
PF6.Locked=true
PF6.Signal=GPIO_Output
PF7.Locked=true
PF7.Signal=GPIO_Output
PF8.GPIOParameters=GPIO_PuPd
PF8.GPIO_PuPd=GPIO_NOPULL
PF8.Locked=true
PF8.Signal=GPIO_Input
PF9.GPIOParameters=GPIO_PuPd
PF9.GPIO_PuPd=GPIO_NOPULL
PF9.Locked=true
PF9.Signal=GPIO_Input
PG0.Signal=FMC_A10
PG1.Signal=FMC_A11
PG10.Mode=NorPsramChipSelect3_3
PG10.Signal=FMC_NE3
PG11.GPIOParameters=GPIO_Speed,GPIO_PuPd
PG11.GPIO_PuPd=GPIO_NOPULL
PG11.GPIO_Speed=GPIO_SPEED_FREQ_VERY_HIGH
PG11.Locked=true
PG11.Signal=GPIO_Output
PG12.Mode=NorPsramChipSelect4_4
PG12.Signal=FMC_NE4
PG13.Locked=true
PG13.Signal=FMC_A24
PG14.Locked=true
PG14.Signal=FMC_A25
PG15.Locked=true
PG15.Signal=GPIO_Output
PG2.Signal=FMC_A12
PG3.Signal=FMC_A13
PG4.Signal=FMC_A14
PG5.Signal=FMC_A15
PG6.Locked=true
PG6.Signal=GPIO_Output
PG7.Locked=true
PG7.Mode=I2C
PG7.Signal=I2C3_SCL
PG8.Locked=true
PG8.Mode=I2C
PG8.Signal=I2C3_SDA
PG9.Mode=NorPsramChipSelect2_2
PG9.Signal=FMC_NE2
PH0-OSC_IN\ (PH0).Mode=HSE-External-Oscillator
PH0-OSC_IN\ (PH0).Signal=RCC_OSC_IN
PH1-OSC_OUT\ (PH1).Mode=HSE-External-Oscillator
PH1-OSC_OUT\ (PH1).Signal=RCC_OSC_OUT
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32L552ZETx
ProjectManager.FirmwarePackage=STM32Cube FW_L5 V1.5.0
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=STM32CubeIDE
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=imc_freertos_app_m33.ioc
ProjectManager.ProjectName=imc_freertos_app_m33
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-HAL-true,2-SystemClock_Config-RCC-false-HAL-false,3-MX_ADC1_Init-ADC1-false-HAL-true,4-MX_FDCAN1_Init-FDCAN1-false-HAL-true,5-MX_FMC_Init-FMC-false-HAL-true,6-MX_I2C1_Init-I2C1-false-HAL-true,7-MX_I2C3_Init-I2C3-false-HAL-true,8-MX_SPI1_Init-SPI1-false-HAL-true,9-MX_SPI2_Init-SPI2-false-HAL-true,10-MX_TIM7_Init-TIM7-false-HAL-true,11-MX_UART4_Init-UART4-false-HAL-true,12-MX_USART1_UART_Init-USART1-false-HAL-true,13-MX_USART2_UART_Init-USART2-false-HAL-true,14-MX_USART3_UART_Init-USART3-false-HAL-true,15-MX_ICACHE_Init-ICACHE-false-HAL-true,16-MX_USB_Device_Init-USB_DEVICE-false-HAL-false,17-MX_GTZC_Init-GTZC-false-HAL-true,18-MX_ADC2_Init-ADC2-false-HAL-true,0-MX_PWR_Init-PWR-false-HAL-true
RCC.ADCFreq_Value=48000000
RCC.AHBCLKDivider=RCC_SYSCLK_DIV2
RCC.AHBFreq_Value=32000000
RCC.APB1Freq_Value=32000000
RCC.APB1TimFreq_Value=32000000
RCC.APB2Freq_Value=32000000
RCC.APB2TimFreq_Value=32000000
RCC.CRSFreq_Value=48000000
RCC.CortexFreq_Value=32000000
RCC.DFSDMFreq_Value=32000000
RCC.FCLKCortexFreq_Value=32000000
RCC.FDCANFreq_Value=64000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=32000000
RCC.HSE_VALUE=16000000
RCC.HSI48_VALUE=48000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=32000000
RCC.I2C2Freq_Value=32000000
RCC.I2C3Freq_Value=32000000
RCC.I2C4Freq_Value=32000000
RCC.IPParameters=ADCFreq_Value,AHBCLKDivider,AHBFreq_Value,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,CRSFreq_Value,CortexFreq_Value,DFSDMFreq_Value,FCLKCortexFreq_Value,FDCANFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI48_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2C4Freq_Value,LPTIM1Freq_Value,LPTIM2Freq_Value,LPTIM3Freq_Value,LPUART1Freq_Value,LSCOPinFreq_Value,LSI_VALUE,MCO1PinFreq_Value,MSI_VALUE,OCTOSPIMFreq_Value,PLLN,PLLPoutputFreq_Value,PLLQ,PLLQoutputFreq_Value,PLLR,PLLRCLKFreq_Value,PLLSAI1N,PLLSAI1PoutputFreq_Value,PLLSAI1QoutputFreq_Value,PLLSAI1RoutputFreq_Value,PLLSAI2PoutputFreq_Value,PLLSourceVirtual,PWRFreq_Value,RNGFreq_Value,RTCFreq_Value,SAI1Freq_Value,SAI2Freq_Value,SDMMCFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,UART5Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USBFreq_Value,VCOInput2Freq_Value,VCOInput3Freq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOSAI1OutputFreq_Value,VCOSAI2OutputFreq_Value,WatchDogFreq_Value
RCC.LPTIM1Freq_Value=32000000
RCC.LPTIM2Freq_Value=32000000
RCC.LPTIM3Freq_Value=32000000
RCC.LPUART1Freq_Value=32000000
RCC.LSCOPinFreq_Value=32000
RCC.LSI_VALUE=32000
RCC.MCO1PinFreq_Value=64000000
RCC.MSI_VALUE=4000000
RCC.OCTOSPIMFreq_Value=64000000
RCC.PLLN=16
RCC.PLLPoutputFreq_Value=36571428.571428575
RCC.PLLQ=RCC_PLLQ_DIV4
RCC.PLLQoutputFreq_Value=64000000
RCC.PLLR=RCC_PLLR_DIV4
RCC.PLLRCLKFreq_Value=64000000
RCC.PLLSAI1N=24
RCC.PLLSAI1PoutputFreq_Value=13714285.714285715
RCC.PLLSAI1QoutputFreq_Value=48000000
RCC.PLLSAI1RoutputFreq_Value=48000000
RCC.PLLSAI2PoutputFreq_Value=4571428.571428572
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.PWRFreq_Value=64000000
RCC.RNGFreq_Value=48000000
RCC.RTCFreq_Value=32000
RCC.SAI1Freq_Value=13714285.714285715
RCC.SAI2Freq_Value=13714285.714285715
RCC.SDMMCFreq_Value=36571428.571428575
RCC.SYSCLKFreq_VALUE=64000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=32000000
RCC.UART5Freq_Value=32000000
RCC.USART1Freq_Value=32000000
RCC.USART2Freq_Value=32000000
RCC.USART3Freq_Value=32000000
RCC.USBFreq_Value=48000000
RCC.VCOInput2Freq_Value=4000000
RCC.VCOInput3Freq_Value=4000000
RCC.VCOInputFreq_Value=16000000
RCC.VCOOutputFreq_Value=256000000
RCC.VCOSAI1OutputFreq_Value=96000000
RCC.VCOSAI2OutputFreq_Value=32000000
RCC.WatchDogFreq_Value=32000
SH.ADCx_IN1.0=ADC1_IN1,IN1-Single-Ended
SH.ADCx_IN1.ConfNb=1
SH.ADCx_IN12.0=ADC1_IN12
SH.ADCx_IN12.ConfNb=1
SH.ADCx_IN13.0=ADC1_IN13
SH.ADCx_IN13.ConfNb=1
SH.ADCx_IN15.0=ADC1_IN15
SH.ADCx_IN15.ConfNb=1
SH.ADCx_IN16.0=ADC1_IN16
SH.ADCx_IN16.ConfNb=1
SH.ADCx_IN2.0=ADC1_IN2
SH.ADCx_IN2.1=ADC2_IN2,IN2-Single-Ended
SH.ADCx_IN2.ConfNb=2
SH.ADCx_IN3.0=ADC1_IN3
SH.ADCx_IN3.ConfNb=1
SH.ADCx_IN4.0=ADC1_IN4
SH.ADCx_IN4.ConfNb=1
SH.FMC_A0.0=FMC_A0,24b-a2
SH.FMC_A0.1=FMC_A0,21b-a1
SH.FMC_A0.2=FMC_A0,20b-a3
SH.FMC_A0.3=FMC_A0,20b-a4
SH.FMC_A0.ConfNb=4
SH.FMC_A1.0=FMC_A1,24b-a2
SH.FMC_A1.1=FMC_A1,21b-a1
SH.FMC_A1.2=FMC_A1,20b-a3
SH.FMC_A1.3=FMC_A1,20b-a4
SH.FMC_A1.ConfNb=4
SH.FMC_A10.0=FMC_A10,24b-a2
SH.FMC_A10.1=FMC_A10,21b-a1
SH.FMC_A10.2=FMC_A10,20b-a3
SH.FMC_A10.3=FMC_A10,20b-a4
SH.FMC_A10.ConfNb=4
SH.FMC_A11.0=FMC_A11,24b-a2
SH.FMC_A11.1=FMC_A11,21b-a1
SH.FMC_A11.2=FMC_A11,20b-a3
SH.FMC_A11.3=FMC_A11,20b-a4
SH.FMC_A11.ConfNb=4
SH.FMC_A12.0=FMC_A12,24b-a2
SH.FMC_A12.1=FMC_A12,21b-a1
SH.FMC_A12.2=FMC_A12,20b-a3
SH.FMC_A12.3=FMC_A12,20b-a4
SH.FMC_A12.ConfNb=4
SH.FMC_A13.0=FMC_A13,24b-a2
SH.FMC_A13.1=FMC_A13,21b-a1
SH.FMC_A13.2=FMC_A13,20b-a3
SH.FMC_A13.3=FMC_A13,20b-a4
SH.FMC_A13.ConfNb=4
SH.FMC_A14.0=FMC_A14,24b-a2
SH.FMC_A14.1=FMC_A14,21b-a1
SH.FMC_A14.2=FMC_A14,20b-a3
SH.FMC_A14.3=FMC_A14,20b-a4
SH.FMC_A14.ConfNb=4
SH.FMC_A15.0=FMC_A15,24b-a2
SH.FMC_A15.1=FMC_A15,21b-a1
SH.FMC_A15.2=FMC_A15,20b-a3
SH.FMC_A15.3=FMC_A15,20b-a4
SH.FMC_A15.ConfNb=4
SH.FMC_A16_CLE.0=FMC_A16,24b-a2
SH.FMC_A16_CLE.1=FMC_A16,21b-a1
SH.FMC_A16_CLE.2=FMC_A16,20b-a3
SH.FMC_A16_CLE.3=FMC_A16,20b-a4
SH.FMC_A16_CLE.ConfNb=4
SH.FMC_A17_ALE.0=FMC_A17,24b-a2
SH.FMC_A17_ALE.1=FMC_A17,21b-a1
SH.FMC_A17_ALE.2=FMC_A17,20b-a3
SH.FMC_A17_ALE.3=FMC_A17,20b-a4
SH.FMC_A17_ALE.ConfNb=4
SH.FMC_A18.0=FMC_A18,24b-a2
SH.FMC_A18.1=FMC_A18,21b-a1
SH.FMC_A18.2=FMC_A18,20b-a3
SH.FMC_A18.3=FMC_A18,20b-a4
SH.FMC_A18.ConfNb=4
SH.FMC_A19.0=FMC_A19,24b-a2
SH.FMC_A19.1=FMC_A19,21b-a1
SH.FMC_A19.2=FMC_A19,20b-a3
SH.FMC_A19.3=FMC_A19,20b-a4
SH.FMC_A19.ConfNb=4
SH.FMC_A2.0=FMC_A2,24b-a2
SH.FMC_A2.1=FMC_A2,21b-a1
SH.FMC_A2.2=FMC_A2,20b-a3
SH.FMC_A2.3=FMC_A2,20b-a4
SH.FMC_A2.ConfNb=4
SH.FMC_A20.0=FMC_A20,24b-a2
SH.FMC_A20.1=FMC_A20,21b-a1
SH.FMC_A20.ConfNb=2
SH.FMC_A21.0=FMC_A21,24b-a2
SH.FMC_A21.ConfNb=1
SH.FMC_A22.0=FMC_A22,24b-a2
SH.FMC_A22.ConfNb=1
SH.FMC_A23.0=FMC_A23,24b-a2
SH.FMC_A23.ConfNb=1
SH.FMC_A24.0=FMC_A24
SH.FMC_A24.ConfNb=1
SH.FMC_A25.0=FMC_A25
SH.FMC_A25.ConfNb=1
SH.FMC_A3.0=FMC_A3,24b-a2
SH.FMC_A3.1=FMC_A3,21b-a1
SH.FMC_A3.2=FMC_A3,20b-a3
SH.FMC_A3.3=FMC_A3,20b-a4
SH.FMC_A3.ConfNb=4
SH.FMC_A4.0=FMC_A4,24b-a2
SH.FMC_A4.1=FMC_A4,21b-a1
SH.FMC_A4.2=FMC_A4,20b-a3
SH.FMC_A4.3=FMC_A4,20b-a4
SH.FMC_A4.ConfNb=4
SH.FMC_A5.0=FMC_A5,24b-a2
SH.FMC_A5.1=FMC_A5,21b-a1
SH.FMC_A5.2=FMC_A5,20b-a3
SH.FMC_A5.3=FMC_A5,20b-a4
SH.FMC_A5.ConfNb=4
SH.FMC_A6.0=FMC_A6,24b-a2
SH.FMC_A6.1=FMC_A6,21b-a1
SH.FMC_A6.2=FMC_A6,20b-a3
SH.FMC_A6.3=FMC_A6,20b-a4
SH.FMC_A6.ConfNb=4
SH.FMC_A7.0=FMC_A7,24b-a2
SH.FMC_A7.1=FMC_A7,21b-a1
SH.FMC_A7.2=FMC_A7,20b-a3
SH.FMC_A7.3=FMC_A7,20b-a4
SH.FMC_A7.ConfNb=4
SH.FMC_A8.0=FMC_A8,24b-a2
SH.FMC_A8.1=FMC_A8,21b-a1
SH.FMC_A8.2=FMC_A8,20b-a3
SH.FMC_A8.3=FMC_A8,20b-a4
SH.FMC_A8.ConfNb=4
SH.FMC_A9.0=FMC_A9,24b-a2
SH.FMC_A9.1=FMC_A9,21b-a1
SH.FMC_A9.2=FMC_A9,20b-a3
SH.FMC_A9.3=FMC_A9,20b-a4
SH.FMC_A9.ConfNb=4
SH.FMC_D0_DA0.0=FMC_D0,16b-d1
SH.FMC_D0_DA0.1=FMC_D0,16b-d2
SH.FMC_D0_DA0.2=FMC_D0,16b-d3
SH.FMC_D0_DA0.3=FMC_D0,16b-d4
SH.FMC_D0_DA0.ConfNb=4
SH.FMC_D10_DA10.0=FMC_D10,16b-d1
SH.FMC_D10_DA10.1=FMC_D10,16b-d2
SH.FMC_D10_DA10.2=FMC_D10,16b-d3
SH.FMC_D10_DA10.3=FMC_D10,16b-d4
SH.FMC_D10_DA10.ConfNb=4
SH.FMC_D11_DA11.0=FMC_D11,16b-d1
SH.FMC_D11_DA11.1=FMC_D11,16b-d2
SH.FMC_D11_DA11.2=FMC_D11,16b-d3
SH.FMC_D11_DA11.3=FMC_D11,16b-d4
SH.FMC_D11_DA11.ConfNb=4
SH.FMC_D12_DA12.0=FMC_D12,16b-d1
SH.FMC_D12_DA12.1=FMC_D12,16b-d2
SH.FMC_D12_DA12.2=FMC_D12,16b-d3
SH.FMC_D12_DA12.3=FMC_D12,16b-d4
SH.FMC_D12_DA12.ConfNb=4
SH.FMC_D13_DA13.0=FMC_D13,16b-d1
SH.FMC_D13_DA13.1=FMC_D13,16b-d2
SH.FMC_D13_DA13.2=FMC_D13,16b-d3
SH.FMC_D13_DA13.3=FMC_D13,16b-d4
SH.FMC_D13_DA13.ConfNb=4
SH.FMC_D14_DA14.0=FMC_D14,16b-d1
SH.FMC_D14_DA14.1=FMC_D14,16b-d2
SH.FMC_D14_DA14.2=FMC_D14,16b-d3
SH.FMC_D14_DA14.3=FMC_D14,16b-d4
SH.FMC_D14_DA14.ConfNb=4
SH.FMC_D15_DA15.0=FMC_D15,16b-d1
SH.FMC_D15_DA15.1=FMC_D15,16b-d2
SH.FMC_D15_DA15.2=FMC_D15,16b-d3
SH.FMC_D15_DA15.3=FMC_D15,16b-d4
SH.FMC_D15_DA15.ConfNb=4
SH.FMC_D1_DA1.0=FMC_D1,16b-d1
SH.FMC_D1_DA1.1=FMC_D1,16b-d2
SH.FMC_D1_DA1.2=FMC_D1,16b-d3
SH.FMC_D1_DA1.3=FMC_D1,16b-d4
SH.FMC_D1_DA1.ConfNb=4
SH.FMC_D2_DA2.0=FMC_D2,16b-d1
SH.FMC_D2_DA2.1=FMC_D2,16b-d2
SH.FMC_D2_DA2.2=FMC_D2,16b-d3
SH.FMC_D2_DA2.3=FMC_D2,16b-d4
SH.FMC_D2_DA2.ConfNb=4
SH.FMC_D3_DA3.0=FMC_D3,16b-d1
SH.FMC_D3_DA3.1=FMC_D3,16b-d2
SH.FMC_D3_DA3.2=FMC_D3,16b-d3
SH.FMC_D3_DA3.3=FMC_D3,16b-d4
SH.FMC_D3_DA3.ConfNb=4
SH.FMC_D4_DA4.0=FMC_D4,16b-d1
SH.FMC_D4_DA4.1=FMC_D4,16b-d2
SH.FMC_D4_DA4.2=FMC_D4,16b-d3
SH.FMC_D4_DA4.3=FMC_D4,16b-d4
SH.FMC_D4_DA4.ConfNb=4
SH.FMC_D5_DA5.0=FMC_D5,16b-d1
SH.FMC_D5_DA5.1=FMC_D5,16b-d2
SH.FMC_D5_DA5.2=FMC_D5,16b-d3
SH.FMC_D5_DA5.3=FMC_D5,16b-d4
SH.FMC_D5_DA5.ConfNb=4
SH.FMC_D6_DA6.0=FMC_D6,16b-d1
SH.FMC_D6_DA6.1=FMC_D6,16b-d2
SH.FMC_D6_DA6.2=FMC_D6,16b-d3
SH.FMC_D6_DA6.3=FMC_D6,16b-d4
SH.FMC_D6_DA6.ConfNb=4
SH.FMC_D7_DA7.0=FMC_D7,16b-d1
SH.FMC_D7_DA7.1=FMC_D7,16b-d2
SH.FMC_D7_DA7.2=FMC_D7,16b-d3
SH.FMC_D7_DA7.3=FMC_D7,16b-d4
SH.FMC_D7_DA7.ConfNb=4
SH.FMC_D8_DA8.0=FMC_D8,16b-d1
SH.FMC_D8_DA8.1=FMC_D8,16b-d2
SH.FMC_D8_DA8.2=FMC_D8,16b-d3
SH.FMC_D8_DA8.3=FMC_D8,16b-d4
SH.FMC_D8_DA8.ConfNb=4
SH.FMC_D9_DA9.0=FMC_D9,16b-d1
SH.FMC_D9_DA9.1=FMC_D9,16b-d2
SH.FMC_D9_DA9.2=FMC_D9,16b-d3
SH.FMC_D9_DA9.3=FMC_D9,16b-d4
SH.FMC_D9_DA9.ConfNb=4
SH.FMC_NBL0.0=FMC_NBL0,2ByteEnable1
SH.FMC_NBL0.1=FMC_NBL0,2ByteEnable2
SH.FMC_NBL0.2=FMC_NBL0,2ByteEnable3
SH.FMC_NBL0.3=FMC_NBL0,2ByteEnable4
SH.FMC_NBL0.ConfNb=4
SH.FMC_NBL1.0=FMC_NBL1,2ByteEnable1
SH.FMC_NBL1.1=FMC_NBL1,2ByteEnable2
SH.FMC_NBL1.2=FMC_NBL1,2ByteEnable3
SH.FMC_NBL1.3=FMC_NBL1,2ByteEnable4
SH.FMC_NBL1.ConfNb=4
SH.FMC_NOE.0=FMC_NOE,Sram1
SH.FMC_NOE.1=FMC_NOE,Sram2
SH.FMC_NOE.2=FMC_NOE,Sram4
SH.FMC_NOE.3=FMC_NOE,Psram3
SH.FMC_NOE.ConfNb=4
SH.FMC_NWE.0=FMC_NWE,Sram1
SH.FMC_NWE.1=FMC_NWE,Sram2
SH.FMC_NWE.2=FMC_NWE,Sram4
SH.FMC_NWE.3=FMC_NWE,Psram3
SH.FMC_NWE.ConfNb=4
SPI1.BaudRatePrescaler=SPI_BAUDRATEPRESCALER_2
SPI1.CalculateBaudRate=16.0 MBits/s
SPI1.Direction=SPI_DIRECTION_2LINES
SPI1.IPParameters=VirtualType,Mode,Direction,CalculateBaudRate,VirtualNSS,BaudRatePrescaler
SPI1.Mode=SPI_MODE_MASTER
SPI1.VirtualNSS=VM_NSSHARD
SPI1.VirtualType=VM_MASTER
SPI2.BaudRatePrescaler=SPI_BAUDRATEPRESCALER_2
SPI2.CalculateBaudRate=16.0 MBits/s
SPI2.Direction=SPI_DIRECTION_2LINES
SPI2.IPParameters=VirtualType,Mode,Direction,CalculateBaudRate,VirtualNSS,BaudRatePrescaler
SPI2.Mode=SPI_MODE_MASTER
SPI2.VirtualNSS=VM_NSSHARD
SPI2.VirtualType=VM_MASTER
USART1.IPParameters=VirtualMode-Asynchronous
USART1.VirtualMode-Asynchronous=VM_ASYNC
USART2.IPParameters=VirtualMode-Asynchronous
USART2.VirtualMode-Asynchronous=VM_ASYNC
USART3.IPParameters=VirtualMode-Asynchronous
USART3.VirtualMode-Asynchronous=VM_ASYNC
USB_DEVICE.CLASS_NAME_FS=CDC
USB_DEVICE.IPParameters=VirtualMode,VirtualModeFS,CLASS_NAME_FS
USB_DEVICE.VirtualMode=Cdc
USB_DEVICE.VirtualModeFS=Cdc_FS
VP_FREERTOS_VS_CMSIS_V2.Mode=CMSIS_V2
VP_FREERTOS_VS_CMSIS_V2.Signal=FREERTOS_VS_CMSIS_V2
VP_GTZC_VS_GTZC_Enable.Mode=GTZC_Enable
VP_GTZC_VS_GTZC_Enable.Signal=GTZC_VS_GTZC_Enable
VP_ICACHE_VS_ICACHE.Mode=DirectMappedCache
VP_ICACHE_VS_ICACHE.Signal=ICACHE_VS_ICACHE
VP_PWR_VS_DBSignals.Mode=DisableDeadBatterySignals
VP_PWR_VS_DBSignals.Signal=PWR_VS_DBSignals
VP_PWR_VS_SECSignals.Mode=Security/Privilege
VP_PWR_VS_SECSignals.Signal=PWR_VS_SECSignals
VP_SYS_VS_tim2.Mode=TIM2
VP_SYS_VS_tim2.Signal=SYS_VS_tim2
VP_TIM7_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM7_VS_ClockSourceINT.Signal=TIM7_VS_ClockSourceINT
VP_USB_DEVICE_VS_USB_DEVICE_CDC_FS.Mode=CDC_FS
VP_USB_DEVICE_VS_USB_DEVICE_CDC_FS.Signal=USB_DEVICE_VS_USB_DEVICE_CDC_FS
board=custom
rtos.0.ip=FREERTOS
isbadioc=false
